10-04 10:55:03 scand: INFO **** BEGIN-SCAN: GROUP='odyssey', SCAN='2020-10-04-165218' ****
10-04 10:55:03 scand: INFO Serial Number: ODY-2391
10-04 10:55:03 scand: INFO Microscope Serial Number: 0910-10226
10-04 10:55:03 scand: INFO Software Version: 2.1.15
10-04 10:55:03 scand: INFO New doc is: <new><in><scangroup>odyssey</scangroup><scan>2020-10-04-165218</scan><channel>700 800</channel><focus>0</focus><resolution>169</resolution><quality>medium</quality><intensity700>6.5</intensity700><intensity800>5</intensity800><size><x0>0</x0><y0>0</y0><x1>9</x1><y1>13</y1></size><comment/></in></new>
10-04 10:55:03 scand: INFO res='1', speed='2'
10-04 10:55:03 scand: INFO ScandScanner: bandwidth=600Hz
10-04 10:55:03 scand: INFO ScandScanner: filter_filename=/usr/local/licor/dsp600Hz_rev2.hex
10-04 10:55:03 scand: INFO DSPDriver::SetMargin: left=0, right=640
10-04 10:55:03 scand: INFO XYZScanStrategy::Init: initialize analog driver
10-04 10:55:03 scand: INFO XYZScanStrategy::Init: initialize DSP driver ... left=0, right=4256
10-04 10:55:03 scand: INFO DSPDriver::SetMargin: left=0, right=4256
10-04 10:55:03 scand: INFO XYZScanStrategy::Init:  left=-387 right=4643 top=0 bottom=6143
10-04 10:55:03 scand: INFO XYZScanStrategy::Init : gain700=2 volts700=170.059 gain800=1 volts800=180.313
10-04 10:55:03 scand: INFO ScandScanner::do_scan: two channels
10-04 10:55:03 paneld: INFO testState: transition from 'init' to 'pause'
10-04 10:55:05 paneld: INFO testState: transition from 'pause' to 'scan'
10-04 10:55:05 scand: INFO Lid opened; Scan paused.
10-04 10:55:05 paneld: INFO testState: transition from 'scan' to 'pause'
10-04 10:55:13 paneld: INFO testState: transition from 'pause' to 'scan'
10-04 11:02:40 scand: INFO cmd='/usr/local/bin/plot-laser-log-file'
10-04 11:02:43 scand: INFO plot-laser-log-file: sn='0910-10226'
10-04 11:02:43 scand: INFO plot-laser-log-file: laser data file='/home/laserlog/laser'
10-04 11:02:43 scand: INFO plot-laser-log-file: laser graphic file='/home/laserlog/laser.png'
10-04 11:02:43 scand: INFO plot-laser-log-file: max current: 700=53.9, 800=31.6
10-04 11:02:43 scand: INFO plot-laser-log-file: MAX: X=4837782, YMin=0, YMax=60
10-04 11:02:43 scand: INFO plot-laser-log-file::plot: hours=1343.8
10-04 11:02:43 scand: INFO plot-laser-log-file::plot: X as hours=1344
10-04 11:02:43 scand: INFO plot-laser-log-file::plot: exponent=3.12839926871781
10-04 11:02:43 scand: INFO plot-laser-log-file::plot: ceil exponent=4
10-04 11:02:43 scand: INFO plot-laser-log-file::plot: NX=4, XX=10000
10-04 11:02:43 scand: INFO plot-laser-log-file::plot: left=59, top=366, right=1061, bottom=64
10-04 11:02:43 scand: INFO
10-04 11:02:43 scand: INFO Laser graphic generation required 3 seconds
10-04 11:02:43 scand: INFO **** END-SCAN: GROUP='odyssey', SCAN='2020-10-04-165218' ****
