05-27 05:08:16 scand: INFO **** BEGIN-SCAN: GROUP='odyssey', SCAN='2021-05-27-203312' ****
05-27 05:08:16 scand: INFO Serial Number: ODY-2447
05-27 05:08:16 scand: INFO Microscope Serial Number: 0912-10070
05-27 05:08:16 scand: INFO Software Version: 2.1.15
05-27 05:08:16 scand: INFO New doc is: <new><in><scangroup>odyssey</scangroup><scan>2021-05-27-203312</scan><channel>700 800</channel><focus>0</focus><resolution>84</resolution><quality>medium</quality><intensity700>2.5</intensity700><intensity800>5.5</intensity800><size><x0>0</x0><y0>0</y0><x1>5</x1><y1>2</y1></size><comment/></in></new>
05-27 05:08:16 scand: INFO res='2', speed='2'
05-27 05:08:16 scand: INFO ScandScanner: bandwidth=1200Hz
05-27 05:08:16 scand: INFO ScandScanner: filter_filename=/usr/local/licor/dsp1200Hz_rev2.hex
05-27 05:08:16 scand: INFO DSPDriver::SetMargin: left=0, right=640
05-27 05:08:16 scand: INFO XYZScanStrategy::Init: initialize analog driver
05-27 05:08:16 scand: INFO XYZScanStrategy::Init: initialize DSP driver ... left=0, right=2360
05-27 05:08:16 scand: INFO DSPDriver::SetMargin: left=0, right=2360
05-27 05:08:16 scand: INFO XYZScanStrategy::Init:  left=-387 right=2750 top=0 bottom=945
05-27 05:08:16 scand: INFO XYZScanStrategy::Init : gain700=0 volts700=165.957 gain800=2 volts800=142.715
05-27 05:08:16 scand: INFO ScandScanner::do_scan: two channels
05-27 05:08:16 paneld: INFO testState: transition from 'init' to 'pause'
05-27 05:08:16 python:  INFO ageOffDataFiles:  Space Requested:  10485760L  Space Available:  62089281536L
05-27 05:08:18 paneld: INFO testState: transition from 'pause' to 'scan'
05-27 05:08:18 scand: INFO Lid opened; Scan paused.
05-27 05:08:18 paneld: INFO testState: transition from 'scan' to 'pause'
05-27 05:08:29 paneld: INFO testState: transition from 'pause' to 'scan'
05-27 05:09:57 scand: INFO cmd='/usr/local/bin/plot-laser-log-file'
05-27 05:09:58 scand: INFO plot-laser-log-file: sn='0912-10070'
05-27 05:09:58 scand: INFO plot-laser-log-file: laser data file='/home/laserlog/laser'
05-27 05:09:58 scand: INFO plot-laser-log-file: laser graphic file='/home/laserlog/laser.png'
05-27 05:09:58 scand: INFO plot-laser-log-file: max current: 700=53.3, 800=32.2
05-27 05:09:58 scand: INFO plot-laser-log-file: MAX: X=2007602, YMin=0, YMax=59
05-27 05:09:58 scand: INFO plot-laser-log-file::plot: hours=557.7
05-27 05:09:58 scand: INFO plot-laser-log-file::plot: X as hours=558
05-27 05:09:58 scand: INFO plot-laser-log-file::plot: exponent=2.74663419893758
05-27 05:09:58 scand: INFO plot-laser-log-file::plot: ceil exponent=3
05-27 05:09:58 scand: INFO plot-laser-log-file::plot: NX=3, XX=1000
05-27 05:09:58 scand: INFO plot-laser-log-file::plot: left=59, top=366, right=1061, bottom=64
05-27 05:09:58 scand: INFO
05-27 05:09:58 scand: INFO Laser graphic generation required 1 seconds
05-27 05:09:58 scand: INFO **** END-SCAN: GROUP='odyssey', SCAN='2021-05-27-203312' ****
