07-12 16:12:32 scand: INFO **** BEGIN-SCAN: GROUP='odyssey', SCAN='2020-07-12-220945' ****
07-12 16:12:32 scand: INFO Serial Number: ODY-2391
07-12 16:12:32 scand: INFO Microscope Serial Number: 0910-10226
07-12 16:12:32 scand: INFO Software Version: 2.1.15
07-12 16:12:32 scand: INFO New doc is: <new><in><scangroup>odyssey</scangroup><scan>2020-07-12-220945</scan><channel>700 800</channel><focus>0</focus><resolution>169</resolution><quality>medium</quality><intensity700>6</intensity700><intensity800>6</intensity800><size><x0>0</x0><y0>0</y0><x1>17</x1><y1>5</y1></size><comment/></in></new>
07-12 16:12:32 scand: INFO res='1', speed='2'
07-12 16:12:32 scand: INFO ScandScanner: bandwidth=600Hz
07-12 16:12:32 scand: INFO ScandScanner: filter_filename=/usr/local/licor/dsp600Hz_rev2.hex
07-12 16:12:32 scand: INFO DSPDriver::SetMargin: left=0, right=640
07-12 16:12:32 scand: INFO XYZScanStrategy::Init: initialize analog driver
07-12 16:12:32 scand: INFO XYZScanStrategy::Init: initialize DSP driver ... left=0, right=8032
07-12 16:12:32 scand: INFO DSPDriver::SetMargin: left=0, right=8032
07-12 16:12:32 scand: INFO XYZScanStrategy::Init:  left=-387 right=8422 top=0 bottom=2363
07-12 16:12:32 scand: INFO XYZScanStrategy::Init : gain700=2 volts700=159.121 gain800=2 volts800=161.855
07-12 16:12:32 scand: INFO ScandScanner::do_scan: two channels
07-12 16:12:32 paneld: INFO testState: transition from 'init' to 'pause'
07-12 16:12:34 paneld: INFO testState: transition from 'pause' to 'scan'
07-12 16:12:34 scand: INFO Lid opened; Scan paused.
07-12 16:12:34 paneld: INFO testState: transition from 'scan' to 'pause'
07-12 16:12:43 paneld: INFO testState: transition from 'pause' to 'scan'
07-12 16:17:35 scand: INFO cmd='/usr/local/bin/plot-laser-log-file'
07-12 16:17:38 scand: INFO plot-laser-log-file: sn='0910-10226'
07-12 16:17:38 scand: INFO plot-laser-log-file: laser data file='/home/laserlog/laser'
07-12 16:17:38 scand: INFO plot-laser-log-file: laser graphic file='/home/laserlog/laser.png'
07-12 16:17:38 scand: INFO plot-laser-log-file: max current: 700=53.9, 800=31.6
07-12 16:17:38 scand: INFO plot-laser-log-file: MAX: X=4490467, YMin=0, YMax=60
07-12 16:17:38 scand: INFO plot-laser-log-file::plot: hours=1247.4
07-12 16:17:38 scand: INFO plot-laser-log-file::plot: X as hours=1248
07-12 16:17:38 scand: INFO plot-laser-log-file::plot: exponent=3.0962145853464
07-12 16:17:38 scand: INFO plot-laser-log-file::plot: ceil exponent=4
07-12 16:17:38 scand: INFO plot-laser-log-file::plot: NX=4, XX=10000
07-12 16:17:38 scand: INFO plot-laser-log-file::plot: left=59, top=366, right=1061, bottom=64
07-12 16:17:38 scand: INFO
07-12 16:17:38 scand: INFO Laser graphic generation required 3 seconds
07-12 16:17:38 scand: INFO **** END-SCAN: GROUP='odyssey', SCAN='2020-07-12-220945' ****
