**A picture containing indoor

Description automatically generated**

**Figure 2 Supplement 1.** Setup for needle probing thickness measurement, using a 30G x 1.4” hypodermic needle (TSK Laboratory, Japan) adapted to the 1 mm spherical indenter (Biomomentum Inc*.*, Laval, QC).